**12 mm Handscraped Laminate**

DETAILED HANDSCRAPED WOOD VISUAL FLOORING

* 12 MM thick x 6.5” wide
* 2G Valinge Click locking system on HDF
* Visuals offered in several species
* Four sided pressed bevel
* All products are hand scraped
* See Rustic Life collection for additional scraped visuals
* AC3 wear layer – heavy residential
* Warranty: 25 years
* Board length: 48 inches
* Packaging - 17.12sf/ctn, 60ctn/plt, 1027.20sf/plt, 16plt/cont, 16,435.2sf/cont (20')
  + Pallet weight – 2390 lbs.

  

Almond

Batula

Cypress